; PSPad code template for Zemax
; Author: François RIGUET (francois.riguet@reosc.com)
; last revision 11/2013
[Macro definition]
%01value%=@E Value,,
%03value%=@E Value,,
%04value%=@E Value,,
%05value%=@E Value,,
%01surface%=@E Surface number,,
%02surface%=@E Surface number,,
%03surface%=@E Surface number,,
%01NSCsurface%=@E Non-sequential surface number,,
%01index%=@E Index,,
%01vector%=@C Vector,,1,1;2;3;4,
%01field%=@E Field,,
%01stdev%=@E Standard deviation,,
%01string%=@E String variable,,string$
%01string1%=@E String variable 1,,string1$
%02string2%=@E String variable 2,,string2$
%01seed%=@E Seed,,
%01x%=@E X,,
%03x%=@E X,,
%02y%=@E Y,,
%04y%=@E Y,,
%05z%=@E Z,,
%01wavelength%=@E Wavelength number,,
%02wavelength%=@E Wavelength number,,
%01vecsubscript%=@E Subscript value (positive),,
%01code%=@E Property code number,,
%02code%=@E Property code number,,
%03code%=@E Property code number,,
%03nposcode%=@C Code,,,1;2;3;4;5;6,
%03argument2%=@E Second argument,,
%02solvcode%=@C Code,,0,0;1;2;3;4;5,
%03solvparam%=@C Parameter,,0,0;1;2;3,
%01parameter%=@E Parameter number,,
%02parameter%=@E Parameter number,,
%03parameter%=@E Parameter number,,
%02item%=@E Item number (1-12),,
%01window%=@E Window,,
%02line%=@E Line,,
%02column%=@E Column (data type),,
%03column%=@E Column,,
%01row%=@E Row (operand number),,
%02config%=@E Configuration number,,
%03data%=@E Data value,,
%02object%=@E Object number,,
%04face%=@E Face number,,
%02detector%=@E Detector number,,
%03pixel%=@E Pixel number,,
%04nsdcdata%=@C Data type,,0,0;1;2;3,
%04nsdddata%=@C Data type,,0,0;1;2,
%01opecode%=@C Operand code,,EFFL,ABCD;ABSO;ACOS;AMAG;ANAC;ANAR;ANAX;ANAY;ANCX;ANCY;ASIN;ASTI;ATAN;AXCL;BFSD;BIOC;BIOD;BLNK;BSER;CEGT;CELT;CENX;CENY;CEVA;CIGT;CILT;CIVA;CMFV;CMGT;CMLT;CMVA;CNAX;CNAY;CNPX;CNPY;CODA;COGT;COLT;COMA;CONF;CONS;COSI;COVA;CTGT;CTLT;CTVA;CVGT;CVIG;CVLT;CVOL;CVVA;DENC;DENF;DIFF;DIMX;DISA;DISC;DISG;DIST;DIVB;DIVI;DLTN;DMFS;DMGT;DMLT;DMVA;DXDX;DXDY;DYDX;DYDY;EFFL;EFLX;EFLY;EFNO;ENDX;ENPP;EPDI;EQUA;ETGT;ETLT;ETVA;EXPD;EXPP;FCGS;FCGT;FCUR;FDMO;FDRE;FICL;FICP;FOUC;FTGT;FTLT;GBPD;GBPP;GBPR;GBPS;GBPW;GBSD;GBSP;GBSR;GBSS;GBSW;GCOS;GENC;GENF;GLCA;GLCB;GLCC;GLCR;GLCX;GLCY;GLCZ;GMTA;GMTS;GMTT;GOTO;GPIM;GPRT;GPRX;GPRY;GPSX;GPSY;GRMN;GRMX;GTCE;HHCN;IMAE;IMSF;INDX;InGT;InLT;InVA;ISFN;LACL;LINV;LOGE;LOGT;LONA;LPTD;MAXX;MCOG;MCOL;MCOV;MINN;MNAB;MNCA;MNCG;MNCT;MNCV;MNDT;MNEA;MNEG;MNET;MNIN;MNPD;MNSD;MSWA;MSWS;MSWT;MTFA;MTFS;MTFT;MTHA;MTHS;MTHT;MXAB;MXCA;MXCG;MXCT;MXCV;MXDT;MXEA;MXEG;MXET;MXIN;MXPD;MXSD;NORD;NORX;NORY;NORZ;NPGT;NPLT;NPVA;NPXG;NPXL;NPXV;NPYG;NPYL;NPYV;NPZG;NPZL;NPZV;NSDC;NSDD;NSRA;NSRM;NSST;NSTR;NTXG;NTXL;NTXV;NTYG;NTYL;NTYV;NTZG;NTZL;NTZV;OBSN;OOFF;OPDC;OPDM;OPDX;OPGT;OPLT;OPTH;OPVA;OSCD;OSUM;PANA;PANB;PANC;PARA;PARB;PARC;PARR;PARX;PARY;PARZ;PATX;PATY;PETC;PETZ;PIMH;PLEN;PMAG;PMGT;PMLT;PMVA;POPD;POWF;POWP;POWR;PRIM;PROB;PROD;QSUM;RAED;RAEN;RAGA;RAGB;RAGC;RAGX;RAGY;RAGZ;RAID;RAIN;RANG;REAA;REAB;REAC;REAR;REAX;REAY;REAZ;RECI;RELI;RENA;RENB;RENC;RETX;RETY;RGLA;RSCE;RSCH;RSRE;RSRH;RWCE;RWCH;RWRE;RWRH;SAGX;SAGY;SFNO;SINE;SKIN;SKIS;SPCH;SPHA;SQRT;SSAG;STHI;STRH;SUMM;SVIG;TANG;TCGT;TCLT;TCVA;TFNO;TGTH;TMAS;TOLR;TOTR;TRAC;TRAD;TRAE;TRAI;TRAR;TRAX;TRAY;TRCX;TRCY;TTGT;TTHI;TTLT;TTVA;UDOP;USYM;VOLU;WFNO;WLEN;XDGT;XDLT;XDVA;XENC;XENF;XNEA;XNEG;XNET;XXEA;XXEG;XXET;YNIP;ZERN;ZPLM;ZTHI,"
%02substringnumber%=@E Sub-string number,,
%01line%=@E Line number,,1
%01expression%=@E Expression,,
%02charnumber%=@E Number of characters,,
%01macro%=@O Macro file,,,Macro files (*.zpl)|*.zpl,",A
%01windownumber%=@E Window number,,
%01dblindex%=@E Index value (0-50),,
%02dblvalue%=@E Value,,
%02stringvalue%=@E String,,
%01color%=@E Color number (0 to 24),,0
%01copysource%=@O Source file,,,File (*.*)|*.*,",A
%02copydest%=@O Destination file,,,File (*.*)|*.*,",A
%01declarename%=@E Variable name,,
%02declaretype%=@C Variable type,,DOUBLE,DOUBLE;INTEGER,
%03declarenumdim%=@C Number of dimensions,,1,1;2;3;4,
%04declaredim1%=@E Dimension 1,,
%05declaredim2%=@E Dimension 2,", ",
%06declaredim3%=@E Dimension 3,", ",
%07declaredim4%=@E Dimension 4,", ",
%01defmerittype%=@C Type (RMS/PV),,0,0;1,
%02defmeritdata%=@C Data (WF/spot/spot x/spot y/spot x+y),,0,0;1;2;3;4,
%03defmeritreference%=@C Reference (centroid/chief/unref),,0,0;1;2,
%04defmeritmethod%=@C Method (Gaussian/rectangular),,0,0;1,
%05defmeritrings%=@E Number of rings,,
%06defmeritarms%=@E Number of arms,,
%07defmeritgrid%=@E Grid size,,
%08defmeritdelete%=@C Delete vignetted rays (no/yes),,0,0;1
%09defmeritaxial%=@C Axial symmetry (auto/no/axial),,-1,-1;0;1,
%10defmeritlateral%=@C Ignore lateral color (no/yes),,0,0;1
%11defmeritstart%=@E Start (-1 auto/operand number),,-1
%12defmeritxweight%=@E X weight,,
%13defmeritoweight%=@E Overall weight,,
%01deleten%=@E Surface Number,,
%01deleteconfig%=@E Configuration number,,
%01deletefile%=@E File name,,
%01deletemco%=@E Operand row,,
%01deletemfo%@E Operand row or ALL,,
%01deleteobjectsurf%=@E Surface number,,
%02deleteobjectobject%=@E Object number,,
%01exportwinnum%=@E Window number,,
%02exportfilename%=@E File name,,
%03exportdelay%=@E Delay (ms),", ",
%00exportcadfilename%=@E File name
%01exportcadvec%=@C File type (IGES/STEP/SAT/STL),,1,0;1;2;3,
%02exportcadvec%=@E Number of spline points,,
%03exportcadvec%=@E First surface,,
%04exportcadvec%=@E Last surface,,
%05exportcadvec%=@E Layer for rays,,
%06exportcadvec%=@E Layer for lens,,
%07exportcadvec%=@C Export dummy surfaces (no/yes),,0,0;1,
%08exportcadvec%=@C Export surfaces as solids (no/yes),,0,0;1,
%09exportcadvec%=@C Ray pattern (XY/X/Y/ring/list/none),,0,0;1;2;3;4;5,
%10exportcadvec%=@E Number of rays,,
%11exportcadvec%=@E Wave number (0 for all),,
%12exportcadvec%=@E Field number (0 for all),,
%13exportcadvec%=@C Delete vignetted rays (no/yes),,1,0;1,
%14exportcadvec%=@E Dummy surface thickness,,
%15exportcadvec%=@C Split rays from NSC sources (no/yes),,0,0;1,
%16exportcadvec%=@C Scatter rays from NSC sources (no/yes),,0,0;1,
%17exportcadvec%=@C Use polarization for NSC rays (no/yes),,0,0;1,
%18exportcadvec%=@E Configuration (0/1-n/n+1/n+2/n+3),,0
%01findfilevariable%=@E Variable to store results in,,TEMPFILE$
%02findfilefilter%=@E Filter,,C:\ZEMAX\*.ZMX,,"
%01FORvariable%=@E Variable,,i
%02FORstart%=@E Start value,,
%03FORstop%=@E Stop value,,
%04FORincrement%=@E Increment,,
%01format%=@E Format,,
%02formatoption%=@C Option,,,EXP;INT;LIT,
%01getvector%=@C Vector number,,1,1;2;3;4,
%02getsurface%=@E Surface number,,
%02getglass%=@E Glass number,,
%01getlsfwave%=@E Wavelength number,,0
%02getlsffield%=@E Field number,,
%03getlsfsampling%=@C Sampling,,,1;2;3;4;5;6;7,
%04getlsfvector%=@C Vector number,,1,1;2;3;4,
%05getlsfmaxradius%=@E Max radial coordinate of LSF,,0
%06getlsfpolar%=@C Use polarization(no/yes),,0,0;1,
%01getmtffreq%=@E Frequency,,
%02getmtfwave%=@E Wavelength number,,0
%03getmtffield%=@E Field number,,
%04getmtfsampling%=@C Sampling,,,1;2;3;4;5;6;7,
%05getmtfvector%=@C Vector number,,1,1;2;3;4,
%06getmtftype%=@C Data type (MTF/real/imaginary/phase/square wave MTF),,1,1;2;3;4;5,
%01getpsfwave%=@E Wavelength number,,0
%02getpsffield%=@E Field number,,
%03getpsfsampling%=@C Sampling,,,1;2;3;4;5;6;7,
%04getpsfvector%=@C Vector number,,1,1;2;3;4,
%05getpsfunnormalized%=@C Normalized PSF,,0,0;1,
%06getpsfphaseflag%=@C Intensity (0) or phase (1),,0,0;1,
%07getpsfimagedelta%=@E Spacing between PSF points (um),,0
%01getsysdata%=@C Data vector number,,1,1;2;3;4,
%01gettexttextfilename%=@E File name,,,,"
%02gettexttype%=@E Type,,,,"
%03gettextsettingsfilename%=@E Settings,,,,"
%04gettextflag%=@C Settings flag,,0,0;1;2,
%01getvardata%=@C Data vector number,,1,1;2;3;4,
%01getzmaxorder%=@E Max order (1 to 37 or 231),,37
%02getzwave%=@E Wavelength number,,
%03getzfield%=@ Field number,,
%04getzsampling%=@C Sampling,,1,1;2;3;4;5;6;7,
%05getzvector%=@C Output vector,,1,1;2;3;4,
%06getzzerntype%=@C Zernike type (fringe/standard/annular),,0,0;1;2,
%07getzepsilon%=@E Annular ratio (for annular Zernike),,
%08getzreference%=@C OPD Reference (chief ray / surface vertex),,0,0;1,
%01glasstmplcode%=@E Code,,
%02glasstmpldata%=@C Data,,,0;1,
%01gbllclsurf1%=@E Surface 1,,
%02gbllclsurf2%=@E Surface 2,,
%03gbllcldirection%=@C Direction (forward/reverse),,,0;1,
%01graphics%=@C Graphics,,,;NOFRAME;OFF,
%01gtextx%=@E X position,,
%02gtexty%=@E Y position,,
%03gtextangle%=@E Angle,,0
%04gtexttext%=@E Text (in quotes) or string variable,,
%01gtextcy%=@E Y position,,
%02gtextctext%=@E Text,,
%01gtitle%=@E Title,,
%01hamnum%=@E Number of cycles (1-99),,1
%02hamalgo%=@C Algorithm (DLS/OD),,0,0;1,
%01IFcondition%=@E Condition,,()
%02IFelse%=@K Else ?,ELSE,
%01SUBname%=@E Subprogram name,,
%01gotolabel%=@E Label,,
%01xpup%=@E X pupil coordinate,,
%02ypup%=@E Y pupil coordinate,,
%01gtemcode%=@E Code number,,
%01lostcode%=@E Code number,,
%01imagepath%=@E String variable containing the full path to the image,,string$
%01solmope%=@E Operand number,,
%03solmcode%=@C Code number,,0,0;1;2;3;4;5;6;7,
%01sosocode%=@C Code number,,0,0;1,
%01tolvope%=@E Tolerance operand number,,
%02tolvcol%=@E Column number,,
%01glasscat%=@E Catalog number (<1 gives all loaded catalogs),,
%01tolope%=@E Tolerance operand,,
%01cmdexe%=@O Executable program,,,Executable program (*.exe)|*.exe,",A
%02cmdargs%=@E Arguments,,
%01convfile%=@O Text file,,,Text file (*.*)|*.*,",A
%02convencoding%=@C Encoding,,,1;2,
%01deltolrow%=@E Tolerance row number,,
%01imaout%=@O Output file,,,Output file (*.bim)|*.bim,",A
%02imain%=@O Input file,,,Input file (*.ima;*.bim)|*.ima;*.bim,",A
%01imgcombsource1%=@O Source image 1,,,Image file (*.bmp;*.jpg)|*.bmp;*.jpg,",A
%02imgcombsource2%=@O Source image 2,,,Image file (*.bmp;*.jpg)|*.bmp;*.jpg,",A
%03imgcombdest%=@O Destination file,,,Image file (*.bmp;*.jpg)|*.bmp;*.jpg,",A
%04imgcombmode%=@C Mode,,LEFTRIGHT,LEFTRIGHT;TOPBOTTOM,"
%01imgextractsource%=@O Source image,,,Image file (*.bmp;*.jpg)|*.bmp;*.jpg,",A
%02imgextractdest%=@O Destination file,,,Image file (*.bmp;*.jpg)|*.bmp;*.jpg,",A
%03imgextractstartx%=@E X start pixel,,
%04imgextractstarty%=@E Y start pixel,,
%05imgextractwidth%=@E Width,,
%06imgextractheight%=@E Height,,
%01imashow%=@O IMA/BIM file,,,File (*.bim;*.ima)|*.bim;*.ima,",A
%01imasumin1%=@O Input BIM file 1,,,BIM file (*.bim)|*.bim,",A
%02imasumin2%=@O Input BIM file 2,,,BIM file (*.bim)|*.bim,",A
%03imasumout%=@O Output BIM file,,,BIM file (*.bim)|*.bim,",A
%01impsurf%=@E Surface number,,
%02impfile%=@O Data file,,,Data file (*.*)|*.*,",A
%01inputprompt%=@E Prompt string,,,,"
%02inputvar%=@E Input variable (add $ for string),,x
%01inssurf%=@E Surface number,,
%01insconf%=@E Configuration number,,
%01insmco%=@E Operand row,,
%01insmfo%=@E Operand row,,
%01insnscsurf%=@E Surface number,,
%02insnscobj%=@E Object number,,
%01instol%=@E Tolerance row,,
%01label%=@E Label number or text,,
%01lineoldx%=@E X start,,
%02lineoldy%=@E Y start,,
%03linenewx%=@E X end,,
%04linenewy%=@E Y end,,
%01loadzarfile%=@O ZAR File,,,Zemax archive (*.zar)|*.zar,",A
%02loadzarpath%=@S Extract path,,
%01detsurf%=@E Surface number,,
%02detobject%=@E Object number,,
%03detfile%=@O Detector file,,,Detector file (*.ddc;*.ddp;*.ddr;*.ddv)|*.ddc;*.ddp;*.ddr;*.ddv,",A
%01lensfile%=@O Lens File,,,Zemax file (*.zmx)|*.zmx,",A
%02lensflag%=@C Append flag,,0,0;1,
%03lenssession%=@C Session flag,,1,0;1,
%02lenssession%=@C Session flag,,1,0;1,
%01meritfile%=@O Merit function File,,,Merit function file (*.mf)|*.mf,",A
%01tolfile%=@O Tolerance File,,,Tolerance file (*.tol)|*.tol,",A
%01l2gsurf1%=@E First surface,,
%02l2gsurf2%=@E Last surface,,
%03l2gref%=@E Reference surface,,
%01lockwin%=@E Window number (0, -1 or n),,
%01facetin%=@O Input CAD file,,,CAD file (*.*)|*.*,",A
%02facetout%=@O Output ASCII file,,,ASCII file (*.txt)|*.txt,",A
%O1makefolder%=@E Folder path,,C:\,,"
%01settingfile%=@O Settings file,,,Settings file (*.txt)|*.txt,",A
%02settingtype%=@C Type,,,DVW_DATA;DVW_DETECTOR;DVW_FILTER;DVW_MAXPLOT;DVW_MINPLOT;DVW_ROWCOL;DVW_SCALE;DVW_SHOW;DVW_SMOOTHING;DVW_SURFACE;DVW_ZPLANE;DVW_ZRD;EXD_DISPLAYSIZE;EXD_FIELD;EXD_FILESIZE;EXD_WAVE;FOO_SURFACE;GBM_FIELDSIZE;GBM_INPUT;GBM_OUTPUT;GBM_RAYS;GBM_ROTATION;GBM_SURFACE;GBM_XPIX;GBM_XSIZ;GBM_YPIX;GBM_YSIZ;HPC_FIELD;HPC_IMAGEDELTA;HPC_IMAGESAMP;HPC_PUPILSAMP;HPC_TYPE;HPC_WAVE;HPS_FIELD;HPS_IMAGEDELTA;HPS_IMAGESAMP;HPS_PUPILSAMP;HPS_TYPE;HPS_WAVE;ILL_DETSIZE;ILL_SMOOTH;ILL_SOURCE;ILL_SURFACE;IMA_FIELD;IMA_IMAGESIZE;IMA_IMANAME;IMA_KRAYS;IMA_NA;IMA_OUTNAME;IMA_SURFACE;ISM_ABERRATIONS;ISM_FIELD;ISM_FIELDHEIGHT;ISM_FLIP;ISM_GUARDBAND;ISM_INPUTFILE;ISM_ISAMP;ISM_OUTPUTFILE;ISM_OVERSAMPLING;ISM_PIXELSIZE;ISM_POLARIZATION;ISM_PSAMP;ISM_PSFX;ISM_PSFY;ISM_REFERENCE;ISM_ROTATE;ISM_SHOWAS;ISM_SUPPRESS;ISM_WAVE;ISM_XSIZE;ISM_YSIZE;LAY_RAYS;LSF_COHERENT;LSF_FIELD;LSF_PLOTSCALE;LSF_POLARIZATION;LSF_SAMP;LSF_SPREAD;LSF_TYPE;LSF_WAVE;MTF_DASH;MTF_FIELD;MTF_MAXF;MTF_POLAR;MTF_SAMP;MTF_SDLI;MTF_SURF;MTF_TYPE;MTF_WAVE;PCI_FIELD;PCI_FILESIZE;PCI_RESAMPLE;PCI_RSDCX;PCI_RSDCY;PCI_RSDLX;PCI_RSDLY;PCI_RSNX;PCI_RSNY;PCI_WAVE;POP_AUTO;POP_BEAMTYPE;POP_COMPUTE;POP_END;POP_FIBERFILE;POP_FIBERTYPE;POP_FIELD;POP_FPARAMn;POP_IGNOREPOL;POP_PARAMn;POP_PEAKIRRAD;POP_POSITION;POP_POWER;POP_SAMPX;POP_SAMPY;POP_SOURCEFILE;POP_START;POP_TILTX;POP_TILTY;POP_WAVE;POP_WIDEX;POP_WIDEY;PSF_FIELD;PSF_IMAGEDELTA;PSF_NORMALIZE;PSF_PLOTSCALE;PSF_POLARIZATION;PSF_ROW;PSF_SAMP;PSF_SURFACE;PSF_TYPE;PSF_WAVE;SHA_ROTX;SHA_ROTY;SHA_ROTZ;SPT_RAYS;WFM_FIELD;WFM_SAMP;WFM_SUBSR;WFM_SUBSX;WFM_SUBSY;WFM_WAVE,
%03settingvalue%=@E Value,,
%01nstrsurf%=@E Surface number,,
%02nstrsource%=@E Source number,,
%03nstrsplit%=@C Split rays ? (0=no),,0,0;1,
%04nstrscatter%=@C Scatter rays ? (0=no),,0,0;1,
%05nstrusepolar%=@C Use polar ? (0=no),,0,0;1,
%06nstrignoreerrors%=@C Ignore errors ? (0=no),,0,0;1,
%07nstrrandomseed%=@E Random seed (0=random seed),,0
%08nstrsave%=@E Save ray data ? (0=no),,1
%09nstrsavefilename%=@E Output data file,,ray_data.zrd,,"
%10nstrfilter%=@C Filter (change n v... by proper value),,,"Bn";"Dn";"En";"Fn";"Gn";"Hn";"Jn";"Ln";"Mn";"On";"Rn";"Sn";"Tn";"Wn";"X_AXYG(n,v)";"X_AXYL(n,v)";"X_AXZG(n,v)";"X_AXZL(n,v)";"X_AYZG(n,v)";"X_AYZL(n,v)";"X_EXT(n,b) ";"X_GHOST(n,b)";"X_HIT(n,b)";"X_HITFACE(n,f)";"X_HITFACE2(n,f,b)";"X_IAGT(n,v)";"X_IALT(n,v)";"X_IRGT(n,v)";"X_IRLT(n,v)";"X_LGT(n,v) ";"X_LLT(n,v)";"X_MGT(n,v)";"X_MLT(n,v)";"X_NGT(n,v)";"X_NLT(n,v)";"X_ORD(n,b)";"X_SCATTER(n,b)";"X_SCATTERF(n,b)";"X_WAVERANGE(n, a, b)";"X_WAVESHIFT(i,j)";"X_XGT(n,v)";"X_XLT(n,v)";"X_YGT(n,v)";"X_YLT(n,v)";"X_ZGT(n,v)";"X_ZLT(n,v)";"Z","
%01open%=@O Text file,,,Text file (*.txt)|*.txt,",A
%01openawintype%=@E Analysis type (3-letter code),,,"
%02openawinfile%=@O Settings file,,,Settings file (*.cfg)|*.cfg,",A
%01optimnumcycles%=@E Number of cycles (1-99),,
%02optimalgo%=@C Algorithm (0: DLS / 1: orthogonal descent),,0,0;1,
%01optreturndata%=@E Data field,,
%02optreturnresult%=@E Result,,
%01outputout%=@E Destination (SCREEN or file),,SCREEN
%02outputappend%=@K Append,", APPEND",
%01paraxonoff%=@C Paraxial ray tracing,,,ON;OFF,
%01pause%=@C Mode,,TIME,'"text"';TIME;THREADS,
%02pausetime%=@E Time (ms),", ",
%01pixx%=@E X coordinate,,
%02pixy%=@E Y coordinate,,
%00plotparam%=@C Plot parameter,,,BANNER;CHECK;COMM1;COMM2;COMM3;COMM4;COMM5;COMM6;DATA;FORMATX;FORMATY;GO;LABEL;LINE;NEW;RANGEX;RANGEY;TICK;TITLE;TITLEX;TITLEY;WINASPECT,
%01plotstring%=@E String (BANNER COMMn TITLE TITLEX TITLEY),", ",,,"
%02plotxinc%=@E X increment (CHECK TICK),", ",
%03plotyinc%=@E Y increment (CHECK TICK),", ",
%04plotxarr%=@E X array (DATA),", ",
%05plotyarr%=@E Y array (DATA),", ",
%06plotnbpts%=@E Number of points (DATA),", ",
%07plotcolor%=@E Color (DATA),", ",
%08plotstyle%=@E Style (DATA),", ",
%09plotoptions%=@E Options (DATA),", ",
%10plotfmtstr%=@E Format string (FORMATX FORMATY),", ",
%11plotx%=@E X position (LABEL),", ",
%12ploty%=@E Y position (LABEL),", ",
%13plotangle%=@E Angle (LABEL),", ",
%14plotsize%=@E Size (LABEL),", ",
%15plotlblstr%=@E String (LABEL),", ",,,"
%16plotx1%=@E X1 (LINE),", ",
%17ploty1%=@E Y1 (LINE),", ",
%18plotx2%=@E X2 (LINE),", ",
%19ploty2%=@E Y2 (LINE),", ",
%20plotminx%=@E Min X (RANGEX),", ",
%21plotmaxx%=@E Max X (RANGEX),", ",
%22plotminy%=@E Min Y (RANGEY),", ",
%23plotmaxy%=@E Max Y (RANGEY),", ",
%24plottype%=@C Window aspect (WINASPECT),", ",,0;1;2;3,
%00plot2dparam%=@C Plot parameter,,,ACTIVECURSOR;ASPECT;COMM1;COMM2;COMM3;COMM4;COMM5;CONFIG;CONTOURINTERVAL;DATA;DISPLAYTYPE;GO;HIDEADDRESS;LOGPLOT;NEW;RANGE;SURFACESCALE;TITLE;WINASPECT,
%01plot2dleft%=@E Left (ACTIVECURSOR),", ",
%02plot2dright%=@E Right (ACTIVECURSOR),", ",
%03plot2dbottom%=@E Bottom (ACTIVECURSOR),", ",
%04plot2dtop%=@E Top (ACTIVECURSOR),", ",
%05plot2dratio%=@E Ratio (ASPECT),", ",
%06plot2dstring%=@E String (COMMn CONTOURINTERVAL TITLE),", ",,,"
%07plot2dconf%=@E Configuration number (CONFIG) (0 for current config/ -1 for all),", ",
%08plot2darray%=@E Array (DATA),", ",
%09plot2ddisp%=@C Display type (DISPLAYTYPE),", ",,1;2;3;4;5;6,
%10plot2dflag%=@C Hide adress flag (HIDEADDRESS),", ",,0;1,
%11plot2dpeak%=@E Peak (LOGPLOT),", ",
%12plot2ddecades%=@E Decades (LOGPLOT),", ",
%13plot2dmin%=@E Min (RANGE),", ",
%14plot2dmax%=@E Max (RANGE),", ",
%15plot2dscale%=@E Scale (SURFACESCALE),", ",
%16plot2dtype%=@C Window aspect (WINASPECT),", ",,0;1;2;3,
%01poldefjx%=@E Jx field magnitude,,0
%02poldefjy%=@E Jy field magnitude,,1
%03poldefphax%=@E Phase x,,0
%04poldefphay%=@E Phase y,,0
%01poltrahx%=@E Normalized object X coordinate,,
%02poltrahy%=@E Normalized object Y coordinate,,
%03poltrapx%=@E Normalized pupil X coordinate,,
%04poltrapy%=@E Normalized pupil X coordinate,,
%05poltrawav%=@E Wavelength number,,
%06poltravec%=@C Output vector,,1,1;2;3;4,
%07poltrasurf%=@E Surface number,,
%01popfile%=@O Output file,,,Output file (*.zbf)|*.zbf,",A
%02popsurf%=@E Last surface,,
%01printout%=@E Text and/or data,,
%01printfile%=@O Text file,,,Text file (*.txt)|*.txt,",A
%01printwinnum%=@E Window number,,
%01pwavn%=@E Wavelength number,,
%01quickfocmode%=@C Mode,,0,0;1;2;3,
%02quickfoccentr%=@C Centroid,,0,0;1,
%01randseed%=@E Seed,,
%01rtrxx%=@E X coordinate,,
%02rtrxy%=@E Y coordinate,,
%03rtrxz%=@E Z coordinate,,
%04rtrxl%=@E L cosine,,
%05rtrxm%=@E M cosine,,
%06rtrxn%=@E N cosine,,
%07rtrxsurf%=@E Start surface number,,
%08rtrxwav%=@E Wavelength number,,
%01readvarlist%=@E Variable list (coma sparated),,"x, y, z"
%01readstr%=@E String,,A$
%01release%=@E Variable name,,
%01renameold%=@O Old file,,OLD$,File (*.*)|*.*,",A
%02renamenew%=@O New file,,NEW$,File (*.*)|*.*,",A
%01savewinnum%=@E Window number,,
%02savewinfile%=@O Text file,,,Text file (*.txt)|*.txt,",A
%01scatter%=@C Scattering,,ON,ON;OFF,
%01state%=@C State,,0,0;1,
%01setaimdatacode%=@C Code,,,1;2;3;4;5;6;7;8,
%02setaimdatavalue%=@E Value,,
%03setdetpix%=@E Pixel number,,
%04setdetdatatype%=@C Data type,,0,0;1;2;3;4,
%05setdetval%=@E Value,,
%04datatype%=@C Data type,,0,0;1;2;3;4;5,
%03param%=@E Parameter,,
%03npropcode%=@E Property code,,
%01setoprow%=@E Row,,
%02setopcol%=@C Column,,,1;2;3;4;5;6;7;8;9;10;11;12;13,
%02value1%=@E Value 1,,
%03value1%=@E Value 1,,
%03value2%=@E Value 2,,
%04value2%=@E Value 2,,
%01textxsize%=@E X size,,70
%02textysize%=@E Y size,,40
%01settolrow%=@E Row,,
%02settolcol%=@C Column,,,1;2;3;4;5;6;7;8;9;10;11;12;13,
%02tolcol%=@C Column,,,0;1;2;3;4;5;6,
%03toldata%=@E Data (operand name for column = 0),,
%01setvarsurfconf%=@E Surface or configuration number,,
%02setvarcode%=@C Code (M for configuration - change n by adequate number),,,R;T;C;G;I;J;K;Pn;D;En;M;Nn;On,
%03setvarstatus%=@E Status,,
%04setvarobjop%=@E Object or operand (for configuration),,
%01vecsize%=@E Maximum vector size (< 18 000 000)
%01dispfile%=@O Image file,,,Image file (*.bmp;*.jpg)|*.bmp;*.jpg,",A
%01showtext%=@O Text file,,,Text file (*.txt)|*.txt,",A
%02showsave%=@E Save flag,,1
%01solve%=@E Solve,,
%02solvtypecode%=@C Code (replace o and p by object and parameter numbers),,,CF;CV;CM;CC;CP;CN;CO;CA;CE;CQ;CR;CG;CZ;TF;TV;TM;TC;TE;TP;TO;TL;TX;TY;TU;TZ;GF;GM;GP;GS;GO;SA;SU;SP;SM;SZ;KF;KP;KZ;PF_p;PP_p;PC_p;PZ_p;HF;HP;EF_e;EP_e;EZ_p;NSC_PX_o;NSC_PY_o;NSC_PZ_o;NSC_PTX_o;NSC_PTY_o;NSC_PTZ_o;NSC_PMAT_o;NSC_MATF_o;NSC_MATM_o;NSC_MATP_o;NSC_MOFF_o;NSC_ZX_o;NSC_ZY_o;NSC_ZZ_o;NSC_ZTX_o;NSC_ZTY_o;NSC_ZTZ_o;NSC_PP_o_p;NSC_ZP_o_p,
%03solvarg1%=@E Argument 1,,
%04solvarg2%=@E Argument 2,,
%05solvarg3%=@E Argument 3,,
%06solvarg4%=@E Argument 4,,
%01tpftpd%=@O Test plate data file,,,Test plate data file (*.tpd)|*.tpd,",A
%02tpflog%=@O Log file,,,Log file (*.dat)|*.dat,",A
%03tpfmethod%=@C Method,,0,0;1;2;3;4,
%04tpfcycles%=@E Number of cycles,,
%01update%=@C Update (replace n by window number),,,ALL;n;EDITORS;MACROS,
%01vecnumber%=@C Vector number,,1,1;2;3;4,
%02vecsubscript%=@E Subscript,,
%01zbffile%=@O ZBF file,,,ZBF file (*.zbf)|*.zbf,",A
%02zbfmultax%=@E Real part x polarization,,
%03zbfmultbx%=@E Imaginary part x polarization,,
%04zbfmultay%=@E Real part y polarization,,
%05zbfmultby%=@E Imaginary part y polarization,,
%02zbfpropvec%=@C Output vector,,1,1;2;3;4,
%02zbfbeam%=@E Beam array (3D),,
%03zbfprop%=@E Property array (1D),,
%02zbfnx%=@E Number of X points (power of 2),,
%03zbfny%=@E Number of Y points (power of 2),,
%04zbfwx%=@E Total width X,,
%05zbfwy%=@E Total width Y,,
%06zbfdecx%=@E X decenter,,
%07zbfdecy%=@E Y decenter,,
%01zbfcoherent%=@C Coherent (1) or incoherent (0) sum,,,0;1,
%02zbffile1%=@O Input file 1,,,ZBF file (*.zbf)|*.zbf,",A
%03zbffile2%=@O Input file 2,,,ZBF file (*.zbf)|*.zbf,",A
%04zbfoutfile%=@O Output file,,,ZBF file (*.zbf)|*.zbf,",A
%02zbfcx%=@E X tilt center,,0
%03zbfcy%=@E Y tilt center,,0
%04zbftx%=@E X tilt slope,,
%05zbfty%=@E Y tilt slope,,
%01zrdappin%=@O Input (appened) file,,,ZRD file (*.zrd)|*.zrd,",A
%02zrdout%=@O Output file,,,ZRD file (*.zrd)|*.zrd,",A
%01zrdfiltin%=@O Input file,,,ZRD file (*.zrd)|*.zrd,",A
%03zrdfilter%=@E Filter string,,,,"
%02zrdsavout%=@O Output file,,,Output file (*.dat)|*.dat,",A
%04zrdobj%=@E Object number,,
%01zrdfile1%=@O Input file 1,,,ZRD file (*.zrd)|*.zrd,",A
%02zrdfile2%=@O Input file 2,,,ZRD file (*.zrd)|*.zrd,",A
%03zrdoutfile%=@O Output file,,,ZRD file (*.zrd)|*.zrd,",A
%1project%=@E Project name ?,,
%2comment%=@E Comment ?,,
%01nsltsurface%=@E Non sequential surface,,1
%02nsltsource%=@E Source number (0=all),,0
%03nsltraysampl%=@C LightningTrace mesh resolution (0=1x/5=1024x),,,0;1;2;3;4;5,
%04nsltedgesampl%=@C (0=1x/4=256x),,,0;1;2;3;4,
%01readskip%=@E Number of characters to skip (<0 = starts from end of file),,
%01aygenrsmxfile%=@O Input Radiant Source model,,,Radiant Source model (*.rmsx)|*.rmsx,",R
%02raygenrayfile%=@O Output ray file,,output_ray_file.sdf,Ray file (*.sdf)|*.sdf,",R
%03raygennumrays%=@E Number of rays,,
%04raygenminazim%=@E Minimum azimuth angle,,
%05raygenmaxazim%=@E Maximum azimuth angle,,
%06raygenminincl%=@E Minimum inclination angle,,
%07raygenmaxincl%=@E Maximum inclination angle,,
%08raygenoriginmeth%=@C Origination method code,,,0;1;2;3;4;5;6;7;8;9;10;11,
%09raygenoriginrad%=@E Origination radius (mm),,
%10raygenspectrumtype%=@C Spectrum type,,,0;1;2;3,
%11raygenarg1%=@E Argument 1,,
%12raygenarg2%=@E Argument 2,,
%13raygenarg3%=@E Argument 3,,
%01topfile%=@O Tolerance options file,,,Tolerance options file (*.top)|*.top,",R
%02toloutfile%=@O Output file,,tolerance_report.txt,Output file (*.*)|*.*,",R
%01zbf2matfile%=@O Input ZBF file,,,ZBF file (*.zbf)|*.zbf,",A
%02matfile%=@O Output MAT file,,output.mat,MAT file (*.mat)|*.mat,",A
%03zbfsurfrange%=@E Surface range flag (0=all surfaces),,0,0;1,
%04zbf2matinteger1%=@E Starting surface number,,
%05zbf2matinteger2%=@E Final surface number,,
%01zrd2matfile%=@O Input ZRD file,,,ZRD file (*.zrd)|*.zrd,",A
%03zrdsavesegment%=@C Save segment flag,,0,0;1,
%04zrd2matinteger1%=@E First ray,,
%05zrd2matinteger2%=@E Last ray,,
%01zrdpbfile%=@O Input ZRD file,,,ZRD file (*.zrd)|*.zrd,",R
%03zrddetector%=@E Detector object number (0=all detectors),,0
%04zrdclear%=@C Clear detector ? (0=no/1=yes),,0,0;1,
%05zrdfilter%=@E Filter string,,,,"
;
;
; Numeric functions
[ABSO |P Absolute value ]
ABSO(%01value%)|
[ACOS |P Arc cosine ]
ACOS(%01value%)|
[APMN |P Minimum aperture radius ]
APMN(%01surface%)|
[APMX |P Maximum aperture radius ]
APMX(%01surface%)|
[APOI |P Ray intensity apodization factor ]
APOI(%01xpup%, %02ypup%)|
[APTP |P Aperture type ]
APTP(%01surface%)|
[APXD |P Aperture x-decenter ]
APXD(%01surface%)|
[APYD |P Aperture y-decenter ]
APYD(%01surface%)|
[ASIN |P Arc sine ]
ASIN(%01value%)|
[ASPR |P Aspect ratio of the graphics device ]
ASPR()|
[ATAN |P Arc tangent ]
ATAN(%01value%)|
[ATYP |P System aperture type ]
ATYP()|
[AVAL |P System aperture value ]
AVAL()|
[CALD |P Return a value from the CALLMACRO buffer ]
CALD(%01index%)|
[CONF |P Current configuration number ]
CONF()|
[CONI |P Conic constant of the surface ]
CONI(%01surface%)|
[COSI |P Cosine ]
COSI(%01value%)|
[CURV |P Curvature of the surface ]
CURV(%01surface%)|
[EDGE |P Edge thickness at the semi-diameter ]
EDGE(%01surface%)|
[EOFF |P End of file flag ]
EOFF()|
[ETIM |P Elapsed time in seconds since last TIMER ]
ETIM()|
[EXPE |P Exponential (base e) ]
EXPE(%01value%)|
[EXPT |P Power of 10 ]
EXPT(%01value%)|
[FICL |P Fiber coupling efficiency ]
FICL(%01vector%)|
[FLDX |P X-angle or height of specified field ]
FLDX(%01field%)|
[FLDY |P Y-angle or height of specified field ]
FLDY(%01field%)|
[FTYP |P Current field type ]
FTYP()|
[FVAN |P Vignetting angle of specified field ]
FVAN(%01field%)|
[FVCX |P X vignetting compression of specified field ]
FVCX(%01field%)|
[FVCY |P Y vignetting compression of specified field ]
FVCY(%01field%)|
[FVDX |P X vignetting decenter of specified field ]
FVDX(%01field%)|
[FVDY |P Y vignetting decenter of specified field ]
FVDY(%01field%)|
[FWGT |P Field weighting of specified field ]
FWGT(%01field%)|
[GABB |P Abbe number of the glass for the specified surface ]
GABB(%01surface%)|
[GAUS |P Random value with a Gaussian distribution ]
GAUS(%01stdev%)|
[GETT |P Numerical value from any open text window ]
GETT(%01window%, %02line%, %03column%)|
[GIND |P Index at d-line of the glass for the specified surface ]
GIND(%01surface%)|
[GLCA |P Global vertex x vector ]
GLCA(%01surface%)|
[GLCB |P Global vertex y vector ]
GLCB(%01surface%)|
[GLCC |P Global vertex z vector ]
GLCC(%01surface%)|
[GLCM |P Value of global coordinates item ]
GLCM(%01surface%, %02item%)|
[GLCX |P Global vertex x-coordinate ]
GLCX(%01surface%)|
[GLCY |P Global vertex y-coordinate ]
GLCY(%01surface%)|
[GLCZ |P Global vertex z-coordinate ]
GLCZ(%01surface%)|
[GNUM |P Number of the glass in the glass catalog ]
GNUM(%01string%)|
[GPAR |P Partial dispersion coefficient of the glass for the specified surface ]
GPAR(%01surface%)|
[GRIN |P Index of refraction at the specified x, y, z position ]
GRIN(%01surface%, %02wavelength%, %03x%, %04y%, %05z%)|
[GTEM |P Data from glass substitution template ]
GTEM(%01gtemcode%)|
[IMAE |P Geometric image analysis efficiency ]
IMAE(%01seed%)|
[INDX |P Index of refraction at the primary wavelength ]
INDX(%01surface%)|
[INTE |P Largest integer not greater than the argument ]
INTE(%01value%)|
[ISMS |P Odd mirror flag ]
ISMS(%01surface%)|
[LOGE |P Base e logarithm ]
LOGE(%01value%)|
[LOGT |P Base 10 logarithm ]
LOGT(%01value%)|
[LOST |P Lost energy following the most recent NSTR trace ]
LOST(%01lostcode%)|
[MAGN |P Square root of x^2+y^2 ]
MAGN(%01x%, %02y%)|
[MAXF |P Maximum radial field ]
MAXF()|
[MAXG |P Number of glasses currently loaded ]
MAXG()|
[MCON |P Extracts data from the Multi-Configuration Editor (extended) ]
MCON(%01row%, %02config%, %03data%)|
[MCOP |P Extracts data from the Multi-Configuration Editor ]
MCOP(%01row%, %02config%)|
[MFCN |P Update lend and merit function ]
MFCN()|
[NCON |P Number of configurations ]
NCON()|
[NFLD |P Number of defined fields ]
NFLD()|
[NOBJ |P Number of defined NSC objects ]
NOBJ(%01NSCsurface%)|
[NPAR |P Parameter value of NSC object ]
NPAR(%01surface%, %02object%, %03parameter%)|
[NPOS |P Position value of NSC object ]
NPOS(%01surface%, %02object%, %03nposcode%)|
[NPRO |P Numeric or string value from the property pages of NSC objects ]
NPRO(%01surface%, %02object%, %03code%, %04face%)|
[NSDC |P Coherent intensity data on detector ]
NSDC(%01surface%, %02detector%, %03pixel%, %04nsdcdata%)|
[NSDD |P Incoherent intensity data on detector ]
NSDD(%01surface%, %02detector%, %03pixel%, %04nsdddata%)|
[NSUR |P Number of defined surfaces ]
NSUR()|
[NWAV |P Number of defined wavelengths ]
NWAV()|
[OBJC |P Object with comment ]
OBJC(%01string%)|
[OCOD |P Optimization operand code ]
OCOD(%01opecode%)|
[ONUM |P optimization operand id number ]
ONUM(%01string%)|
[OPDC |P Optical path difference ]
OPDC()|
[OPER |P Data from Merit Function Editor ]
OPER(%01row%, %02column%)|
[OPEV |P Computes the same value as any optimization operand would ]
OPEV(%01opecode%, int1, int2, data1, data2, data3, data4)|
[OPEW |P Computes the same value as any optimization operand would (extended)]
OPEW(%01opecode%, int1, int2, data1, data2, data3, data4, data5, data6)|
[OPTH |P Optical path length ]
OPTH(%01surface%)|
[PARM |P Parameter value ]
PARM(%01parameter%, %02surface%)|
[PIXX |P Number of X pixels in the image ]
PIXX(%01imagepath%)|
[PIXY |P Number of Y pixels in the image ]
PIXY(%01imagepath%)|
[PMOD |P Paraxial mode ]
PMOD()|
[POWR |P Power (x^y) ]
POWR(%01x%, %02y%)|
[PVHX |P Data1 parameter from the ZPLM optimization operand ]
PVHX()|
[PVHY |P Data2 parameter from the ZPLM optimization operand ]
PVHY()|
[PVPX |P Data3 parameter from the ZPLM optimization operand ]
PVPX()|
[PVPY |P Data4 parameter from the ZPLM optimization operand ]
PVPY()|
[PWAV |P Primary wavelength number ]
PWAV()|
[RADI |P Radius of curvature ]
RADI(%01surface%)|
[RAGL |P Global l direction cosine of the ray following the surface ]
RAGL(%01surface%)|
[RAGM |P Global m direction cosine of the ray following the surface ]
RAGM(%01surface%)|
[RAGN |P Global n direction cosine of the ray following the surface ]
RAGN(%01surface%)|
[RAGX |P Global x coordinate of the ray intercept ]
RAGX(%01surface%)|
[RAGY |P Global y coordinate of the ray intercept ]
RAGY(%01surface%)|
[RAGZ |P Global z coordinate of the ray intercept ]
RAGZ(%01surface%)|
[RAND |P Random number between 0 and input value ]
RAND(%01value%)|
[RANX |P X-direction cosine of the surface normal ]
RANX(%01surface%)|
[RANY |P Y-direction cosine of the surface normal ]
RANY(%01surface%)|
[RANZ |P Z-direction cosine of the surface normal ]
RANZ(%01surface%)|
[RAYE |P Ray-trace error flag ]
RAYE()|
[RAYL |P X-direction cosine of the ray ]
RAYL(%01surface%)|
[RAYM |P Y-direction cosine of the ray ]
RAYM(%01surface%)|
[RAYN |P Z-direction cosine of the ray ]
RAYN(%01surface%)|
[RAYO |P Ray optical path length ]
RAYO(%01surface%)|
[RAYT |P Ray path length ]
RAYT(%01surface%)|
[RAYV |P Vignetted ray flag ]
RAYV()|
[RAYX |P X-coordinate of the ray intercept ]
RAYX(%01surface%)|
[RAYY |P Y-coordinate of the ray intercept ]
RAYY(%01surface%)|
[RAYZ |P Z-coordinate of the ray intercept ]
RAYZ(%01surface%)|
[RELI |P Relative illumination ]
RELI(%01field%)|
[SAGG |P Surface sag ]
SAGG(%01x%, %02y%, %03surface%)|
[SCOM |P String comparison ]
SCOM(%01string1%, %02string2%)|
[SDIA |P Semi-diameter ]
SDIA(%01surface%)|
[SIGN |P Sign ]
SIGN(%01value%)|
[SINE |P Sine ]
SINE(%01value%)|
[SLEN |P String length ]
SLEN(%01string%)|
[SOLM |P Solve type and data ]
SOLM(%01solmope%, %02config%, %03solmcode%)|
[SOLV |P Solve type ]
SOLV(%01surface%, %02solvcode%, %03solvparam%)|
[SOSO |P Surface or object number of a solve ]
SOSO(%01sosocode%)|
[SPRO |P Surface property ]
SPRO(%01surface%, %02code%)|
[SPRX |P Surface property (extended) ]
SPRX(%01surface%, %02code%, %03argument2%)|
[SQRT |P Square root ]
SQRT(%01value%)|
[STDD |P Tilt and decenter ]
STDD(%01surface%, %02parameter%)|
[SURC |P Surface with comment ]
SURC(%01string%)|
[SVAL |P String value ]
SVAL(%01string%)|
[SYPR |P System data ]
SYPR(%01code%)|
[TANG |P Tangent ]
TANG(%01value%)|
[THIC |P Thickness ]
THIC(%01surface%)|
[TMAS |P Total mass ]
TMAS()|
[TOLV |P Tolerance data ]
TOLV(%01tolvope%, %02tolvcol%)|
[UNIT |P Current unit type ]
UNIT()|
[VEC1 |P Value of the VEC1 array ]
VEC1(%01vecsubscript%)|
[VEC2 |P Value of the VEC2 array ]
VEC2(%01vecsubscript%)|
[VEC3 |P Value of the VEC3 array ]
VEC3(%01vecsubscript%)|
[VEC4 |P Value of the VEC4 array ]
VEC4(%01vecsubscript%)|
[VERS |P Zemax version number ]
VERS()|
[WAVL |P Wavelength ]
WAVL(%01wavelength%)|
[WINL |P Number of the most recently opened analysis windows ]
WINL()|
[WINN |P Number of open analysis windows ]
WINN()|
[WWGT |P Wavelength weighting ]
WWGT(%01wavelength%)|
[XMAX |P Maximum x-coordinate in the graphics window ]
XMAX()|
[XMIN |P Minimum x-coordinate in the graphics window ]
XMIN()|
[YMAX |P Maximum y-coordinate in the graphics window ]
YMAX()|
[YMIN |P Minimum y-coordinate in the graphics window ]
YMIN()|
;
;
; String functions
[$BUFFER |B Current string in the lens buffer ]
$BUFFER()|
[$CALLSTR |B String from the CALLMACRO string buffer ]
$CALLSTR(%01index%)|
[$COAT |B Coating name ]
$COAT(%01surface%)|
[$COATINGPATH |B Path name for coating files ]
$COATINGPATH()|
[$COMMENT |B Comment string ]
$COMMENT(%01surface%)|
[$DATAPATH |B Path name for data files ]
$DATAPATH()|
[$DATE |B Date and time ]
$DATE()|
[$EXTENSIONPATH |B Path name for ZEMAX extensions ]
$EXTENSIONPATH()|
[$FILENAME |B Lens file name ]
$FILENAME()|
[$FILEPATH |B Lens file name with the complete path ]
$FILEPATH()|
[$GETSTRING |B Sub-string (space delimiter) ]
$GETSTRING(%01string%, %02substringnumber%)|
[$GETSTRINGC |B Sub-string (comma delimiter) ]
$GETSTRINGC(%01string%, %02substringnumber%)|
[$GLASS |B Glass name ]
$GLASS(%01surface%)|
[$GLASSCATALOG |B Glass catalog name ]
$GLASSCATALOG(%01glasscat%)|
[$GLASSPATH |B Path name for glass catalog files ]
$GLASSPATH()|
[$LEFTSTRING |B Left most n characters ]
$LEFTSTRING(%01string%, %02charnumber%)|
[$LENSNAME |B Lens title ]
$LENSNAME()|
[$MACROPATH |B Path name for macro files ]
$MACROPATH()|
[$NOTE |B Notes information ]
$NOTE(%01line%)|
[$OBJECTPATH |B Path name for NSC object files ]
$OBJECTPATH()|
[$PATHNAME |B Path name ]
$PATHNAME()|
[$PROGRAMPATH |B Path name for program files ]
$PROGRAMPATH()|
[$QUOTE |B Returns double quote character ]
$QUOTE()|
[$RIGHTSTRING |B  Right  most  n  characters ]
$RIGHTSTRING(%01string%, %02charnumber%)|
[$STR |B String formatted expression ]
$STR(%01expression%)|
[$TAB |B Returns tab character ]
$TAB()|
[$TEMPFILENAME |B Temporary file name ]
$TEMPFILENAME|
[$TOLCOMMENT |B Comment for the specified tolerance operand ]
$TOLCOMMENT(%01tolope%)|
[$TOLOPERAND |B Operand name for the specified tolerance operand ]
$TOLOPERAND(%01tolope%)|
[$UNITS |B Lens units ]
$UNITS()|
;
;
; Keywords
[BEEP |R Beep sound ]
BEEP|
[CALLMACRO |R Call another ZPL macro ]
CALLMACRO %01macro%|
[CALLSETDBL |R Set a double precision numeric value ]
CALLSETDBL %01dblindex%, %02dblvalue%|
[CALLSETSTR |R Set string value in buffer ]
CALLSETSTR %01dblindex%, %02stringvalue%|
[CLOSE |R Close an ASCII file ]
CLOSE|
[CLOSEWINDOW |R Suppress the display of the default output window ]
CLOSEWINDOW %01windownumber%|
[COLOR |R Set current pen color ]
COLOR %01color%|
[COMMAND |R Execute a shell command ]
COMMAND %01cmdexe%, %02cmdargs%
[CONVERTFILEFORMAT |R Convert encoding of a text file ]
CONVERTFILEFORMAT %01convfile%, %02convencoding%
[COPYFILE |R Copy source file in a new file ]
COPYFILE %01copysource% %02copydest%|
[DECLARE |R Declare array variable ]
DECLARE %01declarename% %02declaretype% %03declarenumdim% %04declaredim1%%05declaredim2%%06declaredim3%%07declaredim4%|
[DEFAULTMERIT |R Generate a default merit function ]
DEFAULTMERIT %01defmerittype% %02defmeritdata% %03defmeritreference% %04defmeritmethod% %05defmeritrings% %06defmeritarms% %07defmeritgrid% %08defmeritdelete% %09defmeritaxial% %10defmeritlateral% %11defmeritstart% %12defmeritxweight% %13defmeritoweight%|
[DELETE |R Delete a surface ]
DELETE %01deleten%|
[DELETECONFIG |R Delete a configuration ]
DELETECONFIG %01deleteconfig%|
[DELETEFILE |R Delete a file ]
DELETEFILE %01deletefile%|
[DELETEMCO |R Delete a multi-conf operand ]
DELETEMCO %01deletemco%|
[DELETEMFO |R Delete a merit function operand ]
DELETEMFO %01deletemfo%|
[DELETEOBJECT |R Delete an NSC object ]
DELETEOBJECT %01deleteobjectsurf%, %02deleteobjectobject%|
[DELETETOL |R Delete a tolerance ]
DELETETOL %01deltolrow%|
[EXPORTBMP |R Export a graphic window as BMP ]
EXPORTBMP %01exportwinnum%, %02exportfilename%%03exportdelay%|
[EXPORTCAD |R Export a graphic window as CAD ]
VEC1(1) = %01exportcadvec%
VEC1(2) = %02exportcadvec%
VEC1(3) = %03exportcadvec%
VEC1(4) = %04exportcadvec%
VEC1(5) = %05exportcadvec%
VEC1(6) = %06exportcadvec%
VEC1(7) = %07exportcadvec%
VEC1(8) = %08exportcadvec%
VEC1(9) = %09exportcadvec%
VEC1(10) = %10exportcadvec%
VEC1(11) = %11exportcadvec%
VEC1(12) = %12exportcadvec%
VEC1(13) = %13exportcadvec%
VEC1(14) = %14exportcadvec%
VEC1(15) = %15exportcadvec%
VEC1(16) = %16exportcadvec%
VEC1(17) = %17exportcadvec%
VEC1(18) = %18exportcadvec%
EXPORTCAD %00exportcadfilename%|
[EXPORTJPG |R Export a graphic window as JPG ]
EXPORTJPG %01exportwinnum%, %02exportfilename%%03exportdelay%|
[EXPORTWMF |R Export a graphic window as WMF ]
EXPORTWMF %01exportwinnum%, %02exportfilename%|
[FINDFILE |R Find names of files ]
FILTER$ = %02findfilefilter%
FINDFILE %01findfilevariable%, %02findfilefilter%|
[FOR |R FOR statement ]
FOR %01FORvariable%, %02FORstart%, %03FORstop%, %04FORincrement%
    |
NEXT
[FORMAT |R Numerical precision format ]
FORMAT %01format% %02formatoption%|
[GDATE |R Display current date on graphics ]
GDATE|
[GETEXTRADATA |R Get extra data values ]
GETEXTRADATA %01getvector%, %02getsurface%|
[GETGLASSDATA |R Get glass data ]
GETGLASSDATA %01getvector%, %02getglass%|
[GETLSF |R Calculate the geometric LSF ]
GETLSF %01getlsfwave%, %02getlsffield%, %03getlsfsampling%, %04getlsfvector%, %05getlsfmaxradius%, %06getlsfpolar%|
[GETMTF |R Calculate MTF ]
GETMTF %01getmtffreq%, %02getmtfwave%, %03getmtffield%, %04getmtfsampling%, %05getmtfvector%, %06getmtftype%|
[GETPSF |R Calculate PSF ]
GETPSF %01getpsfwave%, %02getpsffield%, %03getpsfsampling%, %04getpsfvector%, %05getpsfunnormalized%, %06getpsfphaseflag%, %07getpsfimagedelta%|
[GETSYSTEMDATA |R Get system data ]
GETSYSTEMDATA %01getsysdata%|
[GETTEXTFILE |R Create a text file ]
GETTEXTFILE %01gettexttextfilename%, %02gettexttype%, %03gettextsettingsfilename%, %04gettextflag%|
[GETVARDATA |R Get variable data ]
GETVARDATA %01getvardata%|
[GETZERNIKE |R Calculate Zernike coefficients ]
GETZERNIKE %01getzmaxorder%, %02getzwave%, %03getzfield%, %04getzsampling%, %05getzvector%, %06getzzerntype%, %07getzepsilon%, %08getzreference%|
[GLASSTEMPLATE |R Glass substitution template ]
GLASSTEMPLATE %01glasstmplcode%, %02glasstmpldata%|
[GLENSNAME |R Use lens name for graphics ]
GLENSNAME|
[GLOBALTOLOCAL |R Convert coord breaks from global to local references ]
GLOBALTOLOCAL %01gbllclsurf1%, %02gbllclsurf2%, %03gbllcldirection%|
[GOSUB |R Sub-program ]
GOSUB %01SUBname%
|
END
SUB %01SUBname%
RETURN
[GOTO |R GOTO statement ]
GOTO %01gotolabel%
|
LABEL %01gotolabel%
[GRAPHICS |R Create standard Zemax graphics ]
GRAPHICS %01graphics%|
[GTEXT |R Graphics labeling ]
GTEXT %01gtextx%, %02gtexty%, %03gtextangle%, %04gtexttext%|
[GTEXTCENT |R Label centering on graphics ]
GTEXTCENT %01gtextcy%, %02gtextctext%|
[GTITLE |R Garaphics title ]
GTITLE %01gtitle%|
[HAMMER |R Hammer optimization ]
HAMMER %01hamnum%, %02hamalgo%|
[IF |R IF statement ]
IF %01IFcondition%
    |
%02IFelse%
ENDIF
[IMA |R Geometric image analysis ]
IMA %01imaout%, %02imain%|
[IMAGECOMBINE |R Combine two images ]
S1$ = %01imgcombsource1%
S2$ = %02imgcombsource2%
D$ = %03imgcombdest%
M$ = %04imgcombmode%
IMAGECOMBINE S1$, S2$, D$, M$|
[IMAGEEXTRACT |R Extract a region from an image ]
S$ = %01imgextractsource%
D$ = %02imgextractdest%
IMAGEEXTRACT S$, D$, %03imgextractstartx%, %04imgextractstarty%, %05imgextractwidth%, %06imgextractheight%|
[IMASHOW |R Display a BIM/IMA file ]
IMASHOW %01imashow%|
[IMASUM |R Sum BIM files ]
IMASUM %01imasumin1%, %02imasumin2%, %03imasumout%|
[IMPORTEXTRADATA |R Import extra data from a file ]
IMPORTEXTRADATA %01impsurf%, %02impfile%|
[INPUT |R Data input ]
INPUT %01inputprompt%, %02inputvar%|
[INSERT |R Insert a surface ]
INSERT %01inssurf%|
[INSERTCONFIG |R Insert a configuration ]
INSERTCONFIG %01insconf%|
[INSERTMCO |R Insert a multi configuration operand ]
INSERTMCO %01insmco%|
[INSERTMFO |R Insert a merit function operand ]
INSERTMFO %01insmfo%|
[INSERTOBJECT |R Insert an NSC object ]
INSERTOBJECT %01insnscsurf%, %02insnscobj%|
[INSERTTOL |R Insert a tolerance ]
INSERTTOL %01instol%|
[LABEL |R Label used with GOTO ]
LABEL %01label%|
[LINE |R Draw a line ]
LINE %01lineoldx%, %02lineoldy%, %03linenewx%, %04linenewy%|
[LOADARCHIVE |R Open a ZAR file ]
LOADARCHIVE %01loadzarfile%, %02loadzarpath%|
[LOADCATALOG |R Reload glass and coating catalogs ]
LOADCATALOG|
[LOADDETECTOR |R Load detector data ]
LOADDETECTOR %01detsurf%, %02detobject%, %03detfile%|
[LOADLENS |R Load a new lens file ]
LOADLENS %01lensfile%, %02lensflag%, %03lenssession%|
[LOADMERIT |R Load a merit function file ]
LOADMERIT %01meritfile%|
[LOADTOLERANCE |R Load a tolerance file ]
LOADTOLERANCE %01tolfile%|
[LOCALTOGLOBAL |R Convert local to global references ]
LOCALTOGLOBAL %01l2gsurf1%, %02l2gsurf2%, %03l2gref%|
[LOCKWINDOW |R Lock windows ]
LOCKWINDOW %01lockwin%|
[MAKEFACETLIST |R Transform a CAD file into ASCII listing ]
MAKEFACETLIST %01facetin%, %02facetout%|
[MAKEFOLDER |R Create a new folder ]
MAKEFOLDER %O1makefolder%|
[MODIFYSETTINGS |R Modify data in a settings file ]
MODIFYSETTINGS %01settingfile%, %02settingtype%, %03settingvalue%|
[NSLT |R Initiate a Non-Sequential LightningTrace ]
NSLT %01nsltsurface%, %02nsltsource%, %03nsltraysampl%, %04nsltedgesampl%|
[NSTR |R Non sequential trace ]
NSTR %01nstrsurf%, %02nstrsource%, %03nstrsplit%, %04nstrscatter%, %05nstrusepolar%, %06nstrignoreerrors%, %07nstrrandomseed%, %08nstrsave%, %09nstrsavefilename%, %10nstrfilter%|
[OPEN |R Open a text file ]
OPEN %01open%|
[OPENANALYSISWINDOW |R Open a new analysis window ]
OPENANALYSISWINDOW %01openawintype%, %02openawinfile%|
[OPTIMIZE |R Optimize ]
OPTIMIZE %01optimnumcycles%, %02optimalgo%|
[OPTRETURN |R Return value from optimization ]
OPTRETURN %01optreturndata%, %02optreturnresult%|
[OUTPUT |R Destination for text output ]
OUTPUT %01outputout%%02outputappend%|
[PARAXIAL |R Paraxial ray tracing ]
PARAXIAL %01paraxonoff%|
[PAUSE |R Pause macro exécution ]
PAUSE %01pause%%02pausetime%|
[PIXEL |R Turn on a pixel on current graphics ]
PIXEL %01pixx%, %02pixy%|
[PLOT |R Create a plot ]
PLOT %00plotparam%%01plotstring%%02plotxinc%%03plotyinc%%04plotxarr%%05plotyarr%%06plotnbpts%%07plotcolor%%08plotstyle%%09plotoptions%%10plotfmtstr%%11plotx%%12ploty%%13plotangle%%14plotsize%%15plotlblstr%%16plotx1%%17ploty1%%18plotx2%%19ploty2%%20plotminx%%21plotmaxx%%22plotminy%%23plotmaxy%%24plottype%|
[PLOT2D |R Create a 2D plot ]
PLOT2D %00plot2dparam%%01plot2dleft%%02plot2dright%%03plot2dbottom%%04plot2dtop%%05plot2dratio%%06plot2dstring%%07plot2dconf%%08plot2darray%%09plot2ddisp%%10plot2dflag%%11plot2dpeak%%12plot2ddecades%%13plot2dmin%%14plot2dmax%%15plot2dscale%%16plot2dtype%|
[POLDEFINE |R Define input polarization state ]
POLDEFINE %01poldefjx%, %02poldefjy%, %03poldefphax%, %04poldefphay%|
[POLTRACE |R Polarization ray tracing ]
POLTRACE %01poltrahx%, %02poltrahy%, %03poltrapx%, %04poltrapy%, %05poltrawav%, %06poltravec%, %07poltrasurf%|
[POP |R Physical optics propagation ]
POP %01popfile%, %02popsurf%|
[PRINT |R Output text and data ]
PRINT %01printout%|
[PRINTFILE |R Print a text file ]
PRINTFILE %01printfile%|
[PRINTWINDOW |R Print a graphic or a text window ]
PRINTWINDOW %01printwinnum%|
[PWAV |R Set the primary wavelength ]
PWAV %01pwavn%|
[QUICKFOCUS |R Adjust last surface's thickness for refocus ]
QUICKFOCUS %01quickfocmode%, %02quickfoccentr%|
[RANDOMIZE |R Change random generator's seed ]
RANDOMIZE %01randseed%|
[RAYGENERATOR |R Run the ray generator ]
RAYGENERATOR %01aygenrsmxfile%, %02raygenrayfile%, %03raygennumrays%, %04raygenminazim%, %05raygenmaxazim%, %06raygenminincl%, %07raygenmaxincl%, %08raygenoriginmeth%, %09raygenoriginrad%, %10raygenspectrumtype%, %11raygenarg1%, %12raygenarg2%, %13raygenarg3%|
[RAYTRACE |R Ray trace ]
RAYTRACE %01poltrahx%, %02poltrahy%, %03poltrapx%, %04poltrapy%, %05poltrawav%|
[RAYTRACEX |R Ray traec from a surface ]
RAYTRACEX %01rtrxx%, %02rtrxy%, %03rtrxz%, %04rtrxl%, %05rtrxm%, %06rtrxn%, %07rtrxsurf%, %08rtrxwav%|
[READ |R Read data ]
READ %01readvarlist%|
[READNEXT |R Read data ]
READNEXT %01readvarlist%|
[READSKIP |R Skip characters of a file ]
READSKIP %01readskip%|
[READSTRING |R Read data and put it in a string ]
READSTRING %01readstr%|
[RELEASE |R Release a variable from memory ]
RELEASE %01release%|
[RELOADOBJECTS |R Reload an NSC object ]
RELOADOBJECTS %01surface%, %02object%|
[REMOVEVARIABLES |R Set all variables to fixed ]
REMOVEVARIABLES|
[RENAMEFILE |R Rename a file ]
RENAMEFILE %01renameold%, %02renamenew%|
[REWIND |R Erase last printed line ]
REWIND|
[SAVEARCHIVE |R Save to a Zemax archive ]
SAVEARCHIVE %01loadzarfile%|
[SAVEDETECTOR |R Save data from an NSC detector ]
SAVEDETECTOR %01surface%, %02object%, %03detfile%|
[SAVELENS |R Save the current lens ]
SAVELENS %01lensfile%, %02lenssession%|
[SAVEMERIT |R Save the merit function to a file ]
SAVEMERIT %01meritfile%|
[SAVETOLERANCE |R Save tolerances to a file ]
SAVETOLERANCE %01tolfile%|
[SAVEWINDOW |R Save window to a file ]
SAVEWINDOW %01savewinnum%, %02savewinfile%|
[SCATTER |R Enable scattering ]
SCATTER %01scatter%|
[SETAIM |R Set the state of ray aiming ]
SETAIM %01state%|
[SETAIMDATA |R Set data for ray aiming ]
SETAIMDATA %01setaimdatacode%, %02setaimdatavalue%|
[SETCONFIG |R Set the configuration ]
SETCONFIG %01deleteconfig%|
[SETDETECTOR |R Set the detector data ]
SETDETECTOR %01surface%, %02object%, %03setdetpix%, %04setdetdatatype%, %05setdetval%|
[SETMCOPERAND |R Set a value in multi-configuration editor ]
SETMCOPERAND %01row%, %02config%, %03value%, %04datatype%|
[SETNSCPARAMETER |R Set a parameter of an NSC object ]
SETNSCPARAMETER %01NSCsurface%, %02object%, %03param%, %04value%|
[SETNSCPOSITION |R Set the position of an NSC object ]
SETNSCPOSITION %01NSCsurface%, %02object%, %03nposcode%, %04value%|
[SETNSCPROPERTY |R Set properties of an NSC object ]
SETNSCPROPERTY %01NSCsurface%, %02object%, %03npropcode%, %04face%, %05value%|
[SETOPERAND |R Set a merit function operand ]
SETOPERAND %01setoprow%, %02setopcol%, %03value%|
[SETSURFACEPROPERTY |R Set properties of a surface ]
SETSURFACEPROPERTY %01surface%, %02code%, %03value1%, %04value2%|
[SETSYSTEMPROPERTY |R Set system properties ]
SETSYSTEMPROPERTY %01code%, %02value1%, %03value2%|
[SETTEXTSIZE |R Change the size of characters ]
SETTEXTSIZE %01textxsize%, %02textysize%|
[SETTOL |R Set data of a tolerance ]
SETTOL %01deltolrow%, %02tolcol%, %03toldata%|
[SETVAR |R Change the status of a variable ]
SETVAR %01setvarsurfconf%, %02setvarcode%, %03setvarstatus%, %04setvarobjop%|
[SETVECSIZE |R Set maximum size of vectors ]
SETVECSIZE %01vecsize%|
[SETVIG |R Set vignetting factors ]
SETVIG|
[SHOWBITMAP |R Display a BMP or JPG image ]
SHOWBITMAP %01dispfile%|
[SHOWFILE |R Display a text file ]
SHOWFILE %01showtext%, %02showsave%|
[SOLVEBEFORESTOP |R Enable ZPL solves prior to the stop ]
SOLVEBEFORESTOP|
[SOLVERETURN |R Return a computed solve value ]
SOLVERETURN %01solve%|
[SOLVETYPE |R Change the solve status ]
SOLVETYPE %01surface%, %02solvtypecode%, %03solvarg1%, %04solvarg2%, %05solvarg3%, %06solvarg4%|
[STOPSURF |R Set the stop surface ]
STOPSURF %01surface%|
[SUB |R Sub-program ]
GOSUB %01SUBname%
    |
END
SUB %01SUBname%
RETURN
[TESTPLATEFIT |R Test plate fit ]
TESTPLATEFIT %01tpftpd%, %02tpflog%, %03tpfmethod%, %04tpfcycles%|
[TOLERANCE |R Run a tolerance analysis ]
TOLERANCE %01topfile%, %02toloutfile%
[TIMER |R Reset internal clock ]
TIMER|
[UNLOCKWINDOW |R Unlock windows ]
UNLOCKWINDOW %01lockwin%|
[UPDATE |R Update data ]
UPDATE %01update%|
[VEC |R Set vector values ]
VEC%01vecnumber% %02vecsubscript%, %03value%|
[XDIFFIA |R Extended diffraction image analysis ]
XDIFFIA %01popfile%, %02imain%|
[ZBF2MAT |R Convert a ZBF file to a Matlab MAT file ]
ZBF2MAT %01zbf2matfile%, %02matfile%, %03zbfsurfrange%, %04zbf2matinteger1%, %05zbf2matinteger2%
[ZBFCLR |R Clear complex amplitude data in a file ]
ZBFCLR %01zbffile%|
[ZBFMULT |R Multiply complex amplitude data in a file ]
ZBFMULT %01zbffile%, %02zbfmultax%, %03zbfmultbx%, %04zbfmultay%, %05zbfmultby%|
[ZBFPROPERTIES |R Put beam data in a vector ]
ZBFPROPERTIES %01zbffile%, %02zbfpropvec%|
[ZBFREAD |R Read a ZBF file ]
ZBFREAD %01zbffile%, %02zbfbeam%, %03zbfprop%|
[ZBFRESAMPLE |R Resample a ZBF file ]
ZBFRESAMPLE %01zbffile%, %02zbfnx%, %03zbfny%, %04zbfwx%, %05zbfwy%, %06zbfdecx%, %07zbfdecy%|
[ZBFSHOW |R Display a ZBF file ]
ZBFSHOW %01zbffile%|
[ZBFSUM |R Sum two ZBF files ]
ZBFSUM %01zbfcoherent%, %02zbffile1%, %03zbffile2%, %04zbfoutfile%|
[ZBFTILT |R Introduce a phase tilt to a ZBF file ]
ZBFTILT %01zbffile%, %02zbfcx%, %03zbfcy%, %04zbftx%, %05zbfty%|
[ZBFWRITE |R Append a ZRD file to another ]
ZRDAPPEND %01zrdappin%, %02zrdout%|
[ZRD2MAT |R Convert a ZRD file to a Matlab MAT file ]
ZRD2MAT %01zrd2matfile%, %02matfile%, %03zrdsavesegment%, %04zrd2matinteger1%, %05zrd2matinteger2%
[ZRDFILTER |R Filter data in a ZRD file ]
ZRDFILTER %01zrdfiltin%, %02zrdout%, %03zrdfilter%|
[ZRDPLAYBACK |R Add ray amplitude data from a ZRD file ]
ZRDPLAYBACK %01zrdpbfile%, %02surface%, %03zrddetector%, %04zrdclear%, %05zrdfilter% 
[ZRDSAVERAYS |R Open a ZRD file and save rays intersecting an object ]
ZRDSAVERAYS %01zrdfiltin%, %02zrdsavout%, %03zrdfilter%, %04zrdobj%|
[ZRDSUM |R Concatenate two ZRD files ]
ZRDSUM %01zrdfile1%, %02zrdfile2%, %03zrdoutfile%|
;
; Useful clips
[HEADER |R Insert header ]
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
! Macro:   %FileName%
! Path:    %FilePath%
! Author:  %UserName% / %Company%
! Date:    %Date%
! Project: %1project%
! Comment: %2comment%
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
|
[SEPARATOR |R Insert separator ]
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
! §
;
;
[Tree Content]
Numeric functions
 ABSO
 ACOS
 APMN
 APMX
 APOI
 APTP
 APXD
 APYD
 ASIN
 ASPR
 ATAN
 ATYP
 AVAL
 CALD
 CONF
 CONI
 COSI
 CURV
 EDGE
 EOFF
 ETIM
 EXPE
 EXPT
 FICL
 FLDX
 FLDY
 FTYP
 FVAN
 FVCX
 FVCY
 FVDX
 FVDY
 FWGT
 GABB
 GAUS
 GETT
 GIND
 GLCA
 GLCB
 GLCC
 GLCM
 GLCX
 GLCY
 GLCZ
 GNUM
 GPAR
 GRIN
 GTEM
 IMAE
 INDX
 INTE
 ISMS
 LOGE
 LOGT
 LOST
 MAGN
 MAXF
 MAXG
 MCON
 MCOP
 MFCN
 NCON
 NFLD
 NOBJ
 NPAR
 NPOS
 NPRO
 NSDC
 NSDD
 NSUR
 NWAV
 OBJC
 OCOD
 ONUM
 OPDC
 OPER
 OPEV
 OPEW
 OPTH
 PARM
 PIXX
 PIXY
 PMOD
 POWR
 PVHX
 PVHY
 PVPX
 PVPY
 PWAV
 RADI
 RAGL
 RAGM
 RAGN
 RAGX
 RAGY
 RAGZ
 RAND
 RANX
 RANY
 RANZ
 RAYE
 RAYL
 RAYM
 RAYN
 RAYO
 RAYT
 RAYV
 RAYX
 RAYY
 RAYZ
 RELI
 SAGG
 SCOM
 SDIA
 SIGN
 SINE
 SLEN
 SOLM
 SOLV
 SOSO
 SPRO
 SPRX
 SQRT
 STDD
 SURC
 SVAL
 SYPR
 TANG
 THIC
 TMAS
 TOLV
 UNIT
 VEC1
 VEC2
 VEC3
 VEC4
 VERS
 WAVL
 WINL
 WINN
 WWGT
 XMAX
 XMIN
 YMAX
 YMIN
String functions
 $BUFFER
 $CALLSTR
 $COAT
 $COATINGPATH
 $COMMENT
 $DATAPATH
 $DATE
 $EXTENSIONPATH
 $FILENAME
 $FILEPATH
 $GETSTRING
 $GETSTRINGC
 $GLASS
 $GLASSCATALOG
 $GLASSPATH
 $LEFTSTRING
 $LENSNAME
 $MACROPATH
 $NOTE
 $OBJECTPATH
 $PATHNAME
 $PROGRAMPATH
 $QUOTE
 $RIGHTSTRING
 $STR
 $TAB
 $TEMPFILENAME
 $TOLCOMMENT
 $TOLOPERAND
 $UNITS
Keywords
 CALLMACRO
 CALLSETDBL
 CALLSETSTR
 CLOSEWINDOW
 COLOR
 COMMAND
 CONVERTFILEFORMAT
 COPYFILE
 DECLARE
 DEFAULTMERIT
 DELETE
 DELETECONFIG
 DELETEMFO
 DELETEOBJECT
 DELETETOL
 EXPORTBMP
 EXPORTCAD
 EXPORTJPG
 EXPORTWMF
 FINDFILE
 FOR
 FORMAT
 GETEXTRADATA
 GETGLASSDATA
 GETLSF
 GETMTF
 GETPSF
 GETSYSTEMDATA
 GETTEXTFILE
 GETVARDATA
 GETZERNIKE
 GLASSTEMPLATE
 GLOBALTOLOCAL
 GOSUB
 GOTO
 GRAPHICS
 GTEXT
 GTEXTCENT
 GTITLE
 HAMMER
 IF
 IMA
 IMAGECOMBINE
 IMAGEEXTRACT
 IMASHOW
 IMASUM
 IMPORTEXTRADATA
 INPUT
 INSERT
 INSERTCONFIG
 INSERTMCO
 INSERTMFO
 INSERTOBJECT
 INSERTTOL
 LABEL
 LINE
 LOADARCHIVE
 LOADDETECTOR
 LOADLENS
 LOADMERIT
 LOADTOLERANCE
 LOCALTOGLOBAL
 LOCKWINDOW
 MAKEFACETLIST
 MAKEFOLDER
 MODIFYSETTINGS
 NSLT
 NSTR
 OPEN
 OPENANALYSISWINDOW
 OPTIMIZE
 OPTRETURN
 OUTPUT
 PARAXIAL
 PAUSE
 PIXEL
 PLOT
 PLOT2D
 POLDEFINE
 POLTRACE
 POP
 PRINT
 PRINTFILE
 PRINTWINDOW
 PWAV
 QUICKFOCUS
 RANDOMIZE
 RAYGENERATOR 
 RAYTRACE
 RAYTRACEX
 READ
 READNEXT
 READSKIP
 READSTRING
 RELEASE
 RELOADOBJECTS
 RENAMEFILE
 SAVEARCHIVE
 SAVEDETECTOR
 SAVELENS
 SAVEMERIT
 SAVETOLERANCE
 SAVEWINDOW
 SCATTER
 SETAIM
 SETAIMDATA
 SETCONFIG
 SETDETECTOR
 SETMCOPERAND
 SETNSCPARAMETER
 SETNSCPOSITION
 SETNSCPROPERTY
 SETOPERAND
 SETSURFACEPROPERTY
 SETSYSTEMPROPERTY
 SETTEXTSIZE
 SETTOL
 SETVAR
 SETVECSIZE
 SHOWBITMAP
 SHOWFILE
 SOLVEBEFORESTOP
 SOLVERETURN
 SOLVETYPE
 STOPSURF
 TESTPLATEFIT
 TOLERANCE
 UNLOCKWINDOW
 UPDATE
 VEC
 XDIFFIA
 ZBF2MAT
 ZBFCLR
 ZBFMULT
 ZBFPROPERTIES
 ZBFREAD
 ZBFRESAMPLE
 ZBFSHOW
 ZBFSUM
 ZBFTILT
 ZRD2MAT
 ZRDAPPEND
 ZRDFILTER
 ZRDPLAYBACK 
 ZRDSAVERAYS
 ZRDSUM
Useful clips
 Header
 Separator
